auto_config_schema.xml
The auto_config_schema.xml file describes the "schema" of a auto-config datasource. You need to edit the schema file according to your auto-config datasource (Registry, INI- or XML-File). The schema file is stored in "%PROGRAM_DIR%\auto_config\" - so you may need admin rights to edit it. The CTI Client "Setup Generator" has a simple editor for the schema file. See CTI Client menu: [File > Create Setup > Dialog "Auto-Configuration"].
Examples for auto_config_schema.xml
Example 1: Auto-config parameters are stored in a central XML file for all users. 1a: If usernames are invalid XML section names 1b: If usernames are valid XML section names 1c: Example for integrated Asterisk Line 1d: Example for integrated Snom, Aastra or Yealink Lines Example 2: Auto-config parameters are stored in a INI file in the user's home drive. Example 3: Auto-config parameters are stored in a XML file in the user's home drive. Example 4: Auto-config parameters are stored in Registry.
Example 1: | Auto-config parameters are stored in a central XML file for all users. Drive "N:" is a public network drive.
Example 1a: | If usernames are invalid XML section names (name contains spaces or other special characters).
N:\cti_client\auto_config_data.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Users> <User Name="Axel Müller" TAPI_LineName="PBX Line 200" /> <User Name="Sanda Jensen" TAPI_LineName="PBX Line 201" /> </Users> <Computers> <Computer Name="PC1" TAPI_LineName="PBX Line 203" /> <Computer Name="PC2" TAPI_LineName="PBX Line 204" /> </Computers> </auto_config>
auto_config_schema.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Sources> <Src1 Path="N:\cti_client\auto_config_data.xml" SubPath="\auto_config\Users\User?Name=%USERNAME%\" /> </Sources> <Schema TAPI_LineName="%Src1%\TAPI_LineName" /> </auto_config>
Comments (valid for all examples):
<Schema TAPI_LineName="%Src1%\TAPI_LineName" />
TAPI_LineName: This is the fix parameter name used inside of application. TAPI_LineName: This is the parameter name inside your auto-config-datasource. Here you can choose an other name if you want. For example: UserTAPIDevice
If you want to run auto-config by computername, you can use the placeholder %COMPUTERNAME% in auto_config_schema.xml. Example: SubPath="\auto_config\Computers\Computer?Name=%COMPUTERNAME%\"
Example 1b: | If usernames are valid XML section names (name contains no spaces or other special characters).
N:\cti_client\auto_config_data.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Users> <amiller TAPI_LineName="PBX Line 200" /> <sjensen TAPI_LineName="PBX Line 201" /> </Users> </auto_config>
auto_config_schema.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Sources> <Src1 Path="N:\cti_client\auto_config_data.xml" SubPath="\auto_config\Users\%USERNAME%\" /> </Sources> <Schema TAPI_LineName="%Src1%\TAPI_LineName" /> </auto_config>
Example 1c: | integrated Asterisk Line
N:\cti_client\auto_config_data.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Users> <User Name="Axel Müller" AsteriskLine_Channel="SIP/203" AsteriskLine_DisplayUsername="Axel Müller" /> </Users> </auto_config>
auto_config_schema.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Sources> <Src1 Path="N:\cti_client\auto_config_data.xml" SubPath="\auto_config\Users\User?Name=%USERNAME%\" /> </Sources> <Schema AsteriskLine_Channel="%Src1%\AsteriskLine_Channel" AsteriskLine_DisplayUsername="%Src1%\AsteriskLine_DisplayUsername" /> </auto_config>
Example 1d: | integrated Snom, Aastra or Yealink Lines
N:\cti_client\auto_config_data.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Users> <User Name="Axel Müller" Phone_IP="192.168.0.3" Phone_Username="test" Phone_Pwd="test" ActionURLs_Port="8080" /> </Users> </auto_config>
auto_config_schema.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Sources> <Src1 Path="N:\cti_client\auto_config_data.xml" SubPath="\auto_config\Users\User?Name=%USERNAME%\" /> </Sources> <Schema Phone_IP="%Src1%\Phone_IP" Phone_Username="%Src1%\Phone_Username" Phone_Pwd="%Src1%\Phone_Pwd" ActionURLs_Port="%Src1%\ActionURLs_Port" /> </auto_config>
Example 2: | Auto-config parameters are stored in a INI file in the user's home drive "H:".
H:\cti_client\auto_config_data.ini:
[auto_config] TAPI_LineName= PBX Line 200
auto_config_schema.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Sources> <Src1 Path="H:\cti_client\auto_config_data.ini" SubPath="\auto_config\" /> </Sources> <Schema TAPI_LineName="%Src1%\TAPI_LineName" /> </auto_config>
Example 3: | Auto-config parameters are stored in a XML file in the user's home drive "H:".
H:\cti_client\auto_config_data.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <data TAPI_LineName="PBX Line 200" /> </auto_config>
auto_config_schema.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Sources> <Src1 Path="H:\cti_client\auto_config_data.xml" SubPath="\auto_config\data\" /> </Sources> <Schema TAPI_LineName="%Src1%\TAPI_LineName" /> </auto_config>
Example 4: Auto-config parameters are stored in Registry.
Registry:
auto_config_schema.xml:
<?xml version="1.0" encoding="ISO-8859-1"?> <auto_config> <Sources> <Src1 Path="HKEY_CURRENT_USER\Software\CTI Client\auto_config\" /> </Sources> <Schema TAPI_LineName="%Src1%\TAPI_LineName" /> </auto_config>